## GPIO NEW TABLE ( Build 20141219 and later)

|  |  |  |  |
| --- | --- | --- | --- |
| **IO index** | **ESP8266 pin** | **IO index** | **ESP8266 pin** |
| 0 [\*] | GPIO16 | 8 | GPIO15 (SPI CS) |
| 1 | GPIO5 | 9 | GPIO3 (UART RX) |
| 2 | GPIO4 | 10 | GPIO1 (UART TX) |
| 3 | GPIO0 | 11 | GPIO9 |
| 4 | GPIO2 | 12 | GPIO10 |
| 5 | GPIO14 (SPI CLK) |  |  |
| 6 | GPIO12 (SPI MISO) |  |  |
| 7 | GPIO13 (SPI MOSI) |  |  |

#### [\*] D0(GPIO16) can only be used as gpio read/write. no interrupt supported. no pwm/i2c/ow supported.